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DISPERSANT 20
DISPERSANT 20 is an extremely effective scale inhibitor, antiprecipitant, and dispersant.

DISPERSANT 20 is a synthetic blend of organic polymers, phosphorus organic derivatives, polymerized phosphates, organic surfactants, and other active ingredients.

USES:
DISPERSANT 20 is recommended for use in cooling water recirculating systems, for the prevention of dispersion of all forms of iron deposits on heat exchangers and all other surfaces.  In addition, it prevents the deposition of tricalcium phosphate, calcium carbonate, calcium sulfate, and other organic deposits.

USE RATIO: 

Approximately 12 to 16 oz. per 1000 gallons of water.

HANDLING:
DISPERSANT 20 is not hazardous to handle in normal use.  However, it should be kept out of eyes and off of skin.  In case of accidental contact, wash thoroughly with copious amounts of water and get medical attention if redness or irritation persists.  KEEP OUT OF REACH  OF CHILDREN.  Keep container closed when not in use.  Do not transfer to improperly marked container.

PACKAGING:
30 gallon drums & 55 gallon drums.
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