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RWT-32A (Acid Type)
COOLING TOWER WATER TREATMENT

RWT-32A is a member of the organophosphorus compounds family marketed by Ryan Chemical Co.

Where as mixtures of polyphosphates and organic chelating agents have been used to achieve an aggregation of properties, RWT-32A provides multiple properties as a single active ingredient.  Specifically, RWT-32A provides the following key properties:

                           SEQUESTION - The ability to complex metal ions at stoichiometric concentrations.

                           DEFLOCCULATION - The ability to disperse solid materials.

                           THRESHOLD EFFECT - The inhibition of precipitation at substoichiometric

                           concentration.

                           HYDROLYTIC STABILITY - The resistance to decomposition in aqueous solutions

                           even at elevated temperatures and extremes in PH.

                           CHLORINE STABILITY - Contains no nitrogen.

The combination of these properties has led to a multitude of applications for RWT-32A, PARTICULARLY FOR SCALE PREVENTION AND CORROSION INHIBITION IN WATER TREATMENT.
                                                 PHYSICAL PROPERTIES OF RWT-32A  
                              Active content........................................................10-12%

                              Color......................................................................Clear to pale yellow.

                              Odor.......................................................................Faint.

                              PH, 1% solution......................................................Less than 2.

                              Specific gravity 20% - 15%....................................10.84 (9.3 lb. / gal.).

                              Crystallization point................................................Below 0 degrees C.

                                                             SOLUBILITY IN:
                              Water.......................................................................Miscible in all proportions.

                              Phosphoric Acid......................................................Miscible in all proportions.

                              Ethylene Glycol.......................................................Miscible in all proportions.

                              Methanol.................................................................50%

USE RATIO: Approximately 16 oz. to 24 oz. per 1000 gallons of water.

PACKAGING: 30 gallon drums & 55 gallon drums.

"WATER TREATING CHEMICALS - WITH SERVICE"
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Office: 800 - 345 – 7208


 www.ryanchemical.com





P.O. Box 406


Chandler, OK  74834








RYAN CHEMICAL Co., Inc.
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